{Definition file for 20X8 PAL}
{Note there are two nominal output pins for each real registered output pin -
for real pin n these are numbered n and n+100 . These correspond to
the two inputs to the exclusive OR gate, so these can be defined
seperately in the .pal file}

40 {fuse-columns}
76 {P-term rows}
20 {inputs}
20 {outputs}

{inputs: pin-number true-column false-column}

2 0 1
3 4 5
4 8 9
5 12 13
6 16 17
7 20 21
8 24 25
9 28 29
10 32 33
11 36 37
14 38 39
15 34 35
16 30 31
17 26 27
18 22 23
19 18 19
20 14 15
21 10 11
22 6 7
23 2 3

{outputs:
pin-number (<0 indicates TS control term) P-term-row-number-list}

14 73-75
-14 72
15 64-65
115 66-67
16 56-57
116 58-59
17 48-49
117 50-51
18 40-41
118 42-43
19 32-33
119 34-35
20 24-25
120 26-27
21 16-17
121 18-19
22 8-9
122 10-11
23 1-3
-23 0

